ELECTRIC WATER BOILER
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SAFELY INSTRUCTIONS
Hints on Connection
• Read all instructions carefully.
• Check the product rating label and make sure the water urn voltage is fit for your outlet voltage before using.
• The plug should be connected to the earth block.
• Do not use the water boiler if the cord or plug is damaged, it should be replaced before using.
• Switch off the button before removing the plug.
• Always switch off before trying to move the water boiler.
[bookmark: _GoBack]• Grasp the plug when you remove it. Do not pull the cord.
• Do not let the power cord hang over edge of a table.
• Place the water boiler securely at the centre of the table.
• Do not switch on the water boiler if the water tank is empty.
• Do not place the water boiler near a gas cooker, electric burner or heated oven.
• Power cord and plug must not touch water in the case of a leakage.
• Please remove the plug from outlet, and cool off the plug before cleaning.
• Press the Switch Off button, and remove the plug after using.
• Do not use this appliance outdoors.
• The appliance requires a 13Amp -16Amp plug.
• The  appliance  is  only  to  be  installed  in  locations  where  it  can  be overseen  by trained personnel.
• Never leave the unit unattended.

Instructions for safe use
• Do not remove the lid while boiling.
• Position the lid so that steam is directed away from the handle.
• Do not carry the urn while it contains water.
• If the appliance is overfilled, boiling water may overflow.
• If the power supply cord is damaged, it must be replaced by the manufacturer or its service agent or a qualified person in order to avoid a hazard.
• This appliance is not int.ended for use by persons (including children) with reduced physical, sensory or mental capabilities, or lack of experience and knowledge, unless they have been given supervision or instruction concerning use of the appliance by a person responsible for their safety.

• Young  children should  be  supervised  to  ensure that they  do  not  play  with  the appliance.
• This appliance can be used by children aged from 8 years and above if they have been given supervision or instruction concerning use of the appliance in a safe way and if they understand the hazards involved. Cleaning and user maintenance shall not  be  made  by  children  unless  they  are  older  than  8  and  supervised.  Keep  the appliance and its cord out of reach of children aged less than 8 years. Children shall not play with the appliance.
• The appliance is not suitable for installation in an area where a water jet could be used. • The appliance must not be cleaned by a water jet. The appliance must not be immersed in water or liquid.

USE AND OPERATIONS
Temperature regulation type
•The temperature controller  has  been  adjusted  before  delivery.  Usually,  the  user does not need to adjust. But the difference of different climates or transportation vibrations  in  different  regions  cause  the  offset  to  the  temperature  controller, resulting  in   low  temperature  water  supply  or  continuous   boiling  of  water  that cannot be controlled. The user can adjust the knob of the temperature controller according to the required temperature. Counterclockwise cooling, clockwise heating. It will meet your requirements for boiling water.

Automatic type
• Plug in the power to start boiling water. At this time, the red indicator light is on,  indicating that the electric water heater is working normally. If the red indicator light  is off, the heat indicator light is on, indicating that the water can be used for drinking. Press the water nozzle can be used to automatically discharge water when you need  the boiling water.

Hints on Boil Dry
•This  device   has  a   preventive  boil  dry  function,   if  the  element  overheats,  the thermostat will cut off the machine automatically. Operating the machine correctly is very important.


If the element does overheat, please just wait few minutes for it to cool down to reset temperature.


CLEANING AND CARE
•The device must be cleaned immediately after the brewing process. Avoid surface drying  of  wort  and  malt  remnants,  as  this  will  significantly  impair  the  cleaning
process.
•  All  stainless  steel  components  can  be  cleaned  using  a  conventional  detergent. Abrasive agents and sponges/brushes that cause scratching are not suitable. Ideally use a pipe cleaner thread to clean the bottom element part.
• When cleaning the brewing vessel ensure that no water spray or moisture comes into  contact  with  the  electrical  components.  The  Plug  must  be  disconnected  for performing cleaning activities.
• Before starting the brewing process, remove all dust and dirt from the device and all internal fittings by means of warm water.
• The valve also needs to be cleaned, all the components like water pipe, cover and false bottom should be cleaned, as this could have a negative impact your brewing results.

TECHNICAL DATA

	Model No.:
	W06MS(D)02-E1 
W10MS(D)02-E1 
W15MS(D)02-E1 

	W20MS(D)02-E4 
W30MS(D)02-E4 

	Voltage:
	110V-120V ~  
220V-240V ~
	220V-240V ~

	Power:
	1500W
	2500W

	Frequency:
	50Hz/60Hz
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